Technical specifications
Supply of a 4x4 vehicle

1. General description
[bookmark: _GoBack]The contractor shall supply one (1) 4x4 vehicle capable for use in:
· prescribed fire operations
· rapid wildfire response
· wildfire suppression and mop-up operations
· operations in remote or difficult-to-access terrain.
The vehicle shall be suitable for forest environments, mountainous terrain, gravel roads, and off-road conditions.
The contractor shall also ensure that the vehicle is legally registered and compliant with national road regulations at the time of delivery.

2. Vehicle specifications
2.1 Vehicle type
· Four-wheel drive utility vehicle suitable for off-road operations
· Capable of towing a trailer-mounted firefighting skid unit
· Suitable for operation on forest roads, gravel tracks, steep slopes, and mountainous terrain
2.2 Dimensions and weight (only indicative range and thresholds)
• Length: approximately 4,800 – 5,500 mm
• Width: 1,800 – 2,000 mm
• Wheelbase: 2,800 – 3,300 mm
• Ground clearance: minimum 220 mm
• Gross Vehicle Weight Rating (GVWR): around a maximum of 2,900 kg
2.3 Engine and drivetrain
• Engine power: minimum 200 HP
• Torque: minimum 350 Nm
• Engine displacement: 3.0 – 4.0 L or equivalent turbocharged engine
• Fuel type: petrol or diesel
• Transmission: automatic 
• Fuel tank capacity: around a minimum of 70 L
Drive system requirements:
• Selectable four-wheel drive system (4×4)
• Drive modes including 2H, 4H, and 4L (low range)
• Rear differential lock or equivalent traction system
2.4 Off-road capability
The vehicle shall be designed for off-road and emergency response operations.
Minimum requirements:
• Ground clearance ≥ 220 mm
• Indicative approach angle ≥ 28°
• Indicative departure angle ≥ 25°
• All-terrain tires suitable for gravel and forest roads
• Heavy-duty suspension suitable for rough terrain
• Front recovery points
2.5 Towing and recovery equipment
• Rear towing hitch 
• Minimum towing capacity: 2,500 kg
The vehicle shall be equipped with a compatible electric recovery winch with the following recommended specifications:
• Line pull capacity: 12,000 – 15,000 lb (≈ 5,400 – 6,800 kg)
• Voltage: 12 V DC
2.6 Exterior equipment
• Lighting suitable for night operation
• Front fog lamps
• Electric side mirrors with indicators
• Cargo area suitable for equipment transport
2.7 Interior equipment
• Seating capacity: minimum four (4) persons including the driver
• Four-door configuration or equivalent access to rear seats 
• Air conditioning
• Power windows
• Central locking system
• Radio or infotainment system with Bluetooth connectivity
2.8 Safety features
Minimum safety equipment shall include:
• Driver and passenger airbags
• Anti-lock braking system (ABS)
• Electronic stability control
• Traction control system
• Hill start assist
• Tire pressure monitoring system
• Fire extinguisher
2.9 Warranty and registration
The vehicle shall be delivered with:
• Minimum warranty of three (3) years or 100,000 km, whichever occurs first
• Vehicle registration and licensing completed in accordance with national regulations
All documentation related to registration, ownership, and warranty shall be provided upon delivery.

3. Non-restriction clause
The technical specifications described in this document define the minimum functional and performance requirements of the requested equipment.
Where specific technical characteristics are indicated, they shall be interpreted as indicative requirements necessary for wildfire response operations and difficult terrain conditions.
Equivalent solutions offering equal or superior performance shall be accepted, provided that the operational requirements, safety standards, and performance specifications described in this document are fully met.



